# Start Up LSM 800

1. Turn on main switch



2. Turn on 2 switches in the rack (System + components)

3. Turn the key (laser I)



4. Start the PC and Zen software

# Shut Down LSM 800

1. Clean objectives and cover the microscope

2. Turn off Zen and the PC

3. Turn the key (laser 0)

4. Turn off 2 switches in the rack (System + components)

5. Switch off the main switch

6. Note time of use and system status in the logbook